**112/01 N13/**

**PANEL CUBICLES - FULLY FRAMED**

* Drawing reference(s):
* Manufacturer and reference: Manufacturer: Cube Install Ltd, The Granary, School Road, Neatishead, Norwich, Norfolk, NR12 8BU,
* Tel: 01692 634000 Email: info@cube-install.com
* Product: **Hive Cubicle System**
* Board/panel/door type: High Density Solid Grade laminate (SGL) with decorative face each side.
* Panel Detail: Full height pilasters/standard height door with overpanel and split divisions joined with low profile aluminium H section.
* Thickness: 12.5mm nominal.
* Edge treatment: All edges radiused and polished (black).
* Depth: 1200mm to 2000mm maximum recommended from face of back wall or rear ducting.
* Floor Clearance: 5mm
* Range height: 2400mm Ceiling Height (std)
* Pedestals: Low profile aluminium giving 5mm floor clearance
* Headrail: High strength continuous extruded aluminium ‘D’ section
* Partition to wall and pilaster fixing: Partitions secured with full length aluminium channels with anti-tamper security fixings for maximum strength and privacy.
* Hinges: High strength aluminium, anti finger trap hinges per door with lift off facility for emergency access and self-closing cams
* Outward opening doors supplied with pull handle and Z section keeps.
* Indicator bolt and keep: Easy slide action lock with integrated buffer and emergency door release facility using security key and red white indicator suitable for users with visual impairment
* Colour/Finish - Fittings: Satin Anodised Aluminium (SAA)
* Colour/Finish - Panels/Doors: From Standard Selection
* Accessories: Matching coat hook, 1 per cubicle